SWIFTFORM® BEST PRACTICE DATA SHEET

Swiftform® is a concrete shuttering product that is made from corrugated plastic reinforced with 3mm diameter bar inserted into the corrugated flute at 140mm centres to create extra strength, then secured by welding 3mm bar to a 5mm strengthening bar. Swiftform® is manufactured in L section, U section, Flat section and specially designed pile caps. The maximum length of a Swiftform® panel is 2.4 metres.
Tools – The only tools required are; Knife for cutting plastic, bolt croppers for cutting 5mm bar, knips for tying wire.
Accessories – Grade plate spacers 12 per M2 for sides or plastic line spacers at every 200 mm depth for sides and tying wire. Swiftform 40/50 Grade plate spacers have been load tested to BS 7973-1:2001 standard. Swiftform can be used in conjunction with heave products.
Joining – Laps are generally 100-200mm, at each joint it is advised that spacers are used over the joint, the joint can also be further secured using tying wire.
Corners – Corners can be supplied however it is very easy to create a corner by bending the 5mm bar and plastic by hand, (creating a corner from L section the 3mm bar on the toe needs to be cut where the corner is to be created)
Pile caps – All pile caps, bases and pads are specifically designed to suit. All supplied with drawings to suit appropriate kit of parts.
U Section – No blinding is required when using U section, it’s easy to cut around protruding piles using just a knife and knips. 
L section- A toe generally 50mm is put on the bottom of the section. The toe can be put facing out to help secure when backfilling, or facing in if putting into a dug out trench.
Estimating – Swiftform® staff can produce a full take off of requirements, including the design of the pile caps. Take offs generally allow 10% extra for laps and corners and beams going in to pile caps, quantities are rounded up the nearest 2.4 metre panel. We can also estimate the quantity of accessories required.
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